{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["第1页"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第1页","index":0,"n_rows":23,"n_cols":36,"rows_kept":23,"merged":[[0,0,23,0],[0,1,0,31],[0,32,23,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,10,1],[9,3,9,8],[9,9,9,12],[9,16,9,25],[9,26,9,31],[10,3,10,8],[10,9,10,12],[10,16,10,25],[10,26,10,31],[11,1,16,1],[11,3,11,8],[11,9,11,12],[11,16,11,25],[11,26,11,31],[12,3,12,8],[12,9,12,12],[12,16,12,25],[12,26,12,31],[13,3,13,8],[13,9,13,12],[13,16,13,25],[13,26,13,31],[14,3,14,8],[14,9,14,12],[14,16,14,25],[14,26,14,31],[15,3,15,8],[15,9,15,12],[15,16,15,25],[15,26,15,31],[16,3,16,8],[16,9,16,12],[16,16,16,25],[16,26,16,31],[17,1,19,5],[17,6,19,15],[17,16,19,16],[17,17,17,21],[17,22,17,31],[18,17,18,21],[18,22,18,31],[19,17,19,31],[20,1,22,5],[20,6,22,15],[20,16,22,16],[20,17,20,31],[21,17,21,21],[21,22,21,31],[22,17,22,31],[23,1,23,31]],"flags":["formulas_cached_only"]}
[]
[null,"消防水箱安装和消防水池施工检验批质量验收记录"]
[null,"GD-C3-51631",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"建筑给水排水及供暖-自动喷水灭火系统",{"$nulls":4},"分项工程\r\n名称",null,null,"供水设施安装与施工"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-51631 消防水箱安装和消防水池施工检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"《自动喷水灭火系统工程施工及验收规范》GB50261-2017"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"主控项目",1,"消防水池、水箱的施工和安装符合相关技术标准规定",{"$nulls":5},"第4.3.1条",{"$nulls":4},"/"]
[null,null,2,"钢筋混凝土消防水池或消防水箱的进水管的进、出管安装要求",{"$nulls":5},"第4.3.2条",{"$nulls":4},"/"]
[null,"一般项目",1,"消防水箱、水池的容积和安装位置符合设计要求；池(箱)外壁净距、通道宽度、顶板净空高度等检修维护相关的空间尺寸要求",{"$nulls":5},"第4.3.3条",{"$nulls":4},"/"]
[null,null,2,"消防水池，高位消防水箱的溢流管、泄水管不得与生产或生活用水的排水系统直接相连，应采用间接排水方式",{"$nulls":5},"第4.3.4条",{"$nulls":4},"/"]
[null,null,3,"高位消防水箱、消防水池的人孔宜密闭。通气管、溢流管应有防止昆虫及小动物爬入水池（箱）的措施",{"$nulls":5},"第4.3.5条",{"$nulls":4},"/"]
[null,null,4,"当高位消防水箱、消防水池与其他用途的水箱、水池合用时，应复核有效的消防水量，满足设计要求，并应设有防止消防用水被他用的措施",{"$nulls":5},"第4.3.6条",{"$nulls":4},"/"]
[null,null,5,"高位消防水箱、消防水池的进水管、出水管上应设置带有指示启闭装置的阀门",{"$nulls":5},"第4.3.7条",{"$nulls":4},"/"]
[null,null,6,"高位消防水箱的出水管上应设置防止消防用水倒流进入高位消防水箱的止回阀",{"$nulls":5},"第4.3.8条",{"$nulls":4},"/"]
[null,"施工单位\r\n检查结果",{"$nulls":15},"施工员："]
[{"$nulls":17},"质量员："]
[{"$nulls":17},"年  月  日"]
[null,"监理单位\r\n验收结论"]
[{"$nulls":17},"专业监理工程师："]
[{"$nulls":17},"年  月  日"]