{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["主推型号"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"主推型号","index":0,"n_rows":109,"n_cols":6,"rows_kept":109,"flags":["formulas_cached_only"]}
[null,"主推型号","封装","描述","最小包装","特别说明"]
[null,"第一类  BCT4XXX  模拟开关系列",null,"电话：075582542001 82574660手机：13360063621"]
[null,"模拟开关  Analog Switch"]
[null,"BCT4157EXT","SC70-6","Sigle SPDT AnalogSwitch 300MHz ","3K/Reel","兼容FSA3157/4157"]
[null,"BCT4268ETB ","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  0.4ohms","3K/Reel","兼容FSA2268、SGM2268"]
[null,"BCT4223ETB ","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  0.4ohms","3K/Reel","兼容PI3A223、NLAS5223"]
[null,"BCT4222AETB ","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  720MHz","3K/Reel","适用于USB2.0的高速开关，兼容NLAS7222,FSUSB30"]
[null,"BCT4222BETB","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  300MHz","3K/Reel","兼容BCT4222A"]
[null,"BCT4222CEAB ","MSOP-10","Dual  SPDTAnalogSwitch  720MHz","3K/Reel","适用于USB2.0的高速开关"]
[null,"BCT4227ETB","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch 720MHz","3K/Reel","适用于USB2.0的高速开关"]
[null,"BCT4717ETB","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  300MHz","3K/Reel","兼容MAX4717ETB、NLAS4717FCT、SGM4717"]
[null,"BCT4599ETE","QFN3x3-16","Quad  SPDTAnalogSwitch  300MHz","3K/Reel","四通道开关，兼容SGM44599、NLAS44599、SGM44599"]
[null,"BCT4699ETE ","QFN3x3-16","Quad  SPDTAnalogSwitch  0.3ohms","3K/Reel","四通道开关，兼容FSA2467、PI3A412、NLAS3699"]
[null,"BCT4121EPT-TR","QFN1.6x1,6-6","Dual SPST AnalogSwitch","3K/Reel","双通道开关，抗class D 纹波"]
[null,"BCT4321N ETB-TR","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  720MHz/-2V","3K/Reel","兼容FSA321，For Micro-USB，USB/Audio switch"]
[null,"BCT4321A ETB-TR","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  720MHz/-0.6V","3K/Reel","兼容FSA321，For Micro-USB，USB/Audio switch"]
[null,"BCT4321B ETB-TR","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  300MHz/-0.6V","3K/Reel","兼容FSA321，For Micro-USB，USB/Audio switch"]
[null,"BCT4322 ETB-TR","QFN1.4x1.8-10","Dual  SPDT AnalogSwitch  720MHz/-0.6V","3K/Reel","兼容FSA321，For Micro-USB，USB/Audio switch"]
[null,"BCT4254NETP-TR","QFN2.5x2.5-16","Dual SP3T AnalogSwitch 720MHz/-2V","3K/Reel","USB/UART/Audio Switch,  For Micro-USB"]
[null,"BCT4252ETP-TR","QFN2.5x2.5-16","Dual SP3T AnalogSwitch 720MHz/-0.6V","3K/Reel","USB/UART/Audio Switch,  For Micro-USB"]
[]
[null,"双SIM卡开关  Dual SIM Card Manager Switch "]
[null,"BCT4302B-TR","QFN3x3-20","Dual SIM Card Controller","3K/Reel","针对MTK平台、展讯SC6600L7平台等"]
[null,"BCT4303ITP-TR","QFN3x3-20","Dual SIM Card Controller","3K/Reel","适用于更多平台，宽范围的VIO"]
[null,"BCT4306EGI-TR","QFN4x4-28","Dual Mode SIM/UIM Card Controller ","3K/Reel","双模双待SIM/UIM控制器,可以支持任意模式基带作为主控"]
[null,"BCT4558ETP-TR","QFN3x3-20","Dual SIM Card Controller","3K/Reel","针对高通WCDMA平台"]
[]
[null,"第二类  BCT3XXX  LED驱动系列"]
[null,"炫彩灯驱动  Glaring LED Driver"]
[null,"BCT3288AEGG-TR","QFN4x4-24","16channel 64steps LED driver with SPI control","3K/Reel","是3288的升级版，完全兼容3288,同时增加了群选地址位、去除IO毛刺等功能"]
[null,"BCT3299EGG-TR","QFN4x4-24","16channel 256steps LED driver with SPI control","3K/Reel","是3288A的升级版，兼容3288；256个亮度等级、内置RAM、内置音乐随动"]
[null,"BCT3286EGI-TR","QFN4x4-28","Audio Modulated Matrix(10x10/11x9/12x8) &32RGB LED driver","3K/Reel","带音频输入检测，可驱动多至10X10、11x9、12x8矩阵灯或32个RGB灯，产生丰富的视觉效果；内置RAM，内置呼吸、游标、RGB配色方案等模式，可以与主机free."]
[null,"BCT3119","QFN4x4-24","9 channel 64steps LED driver with SPI control"]
[]
[null,"白光驱动   LED Driver"]
[null,"BCT3220ELA-TR    ","DFN2x2-8","既共阳又共阴 4 LED Driver","3K/Reel","4路并联背光驱动"]
[null,"BCT3221EGE-TR ","QFN3x3-16","既共阳又共阴 4 LED Driver","3K/Reel","当作为共阳驱动时，兼容RP1364、RT9364"]
[null,"BCT3222ETB-TR","DFN3x3-10","既共阳又共阴 6 LED Driver","3K/Reel","6路并联背光驱动"]
[null,"BCT3223ETB-TR","DFN3x3-10","共阳 6 LED Driver","3K/Reel","6路并联背光驱动"]
[null,"BCT3228ETE-TR","QFN4x4-24","共阳8 LED Driver","3K/Reel","8路并联背光驱动"]
[null,"BCT3256","QFN3x3-16","6路并联共阳",null,"AW9356的替代"]
[null,"BCT3258","QFN3x3-16","8路并联共阳",null,"AW9358的替代"]
[null,"BCT3661ETT-TR","QFN2x2-6","LED Driver up to 10Series","3K/Reel","10路串联背光驱动"]
[null,"BCT3660","QFN2x2-6","8路串联共阳",null,"TI61161的兼容方案"]
[null,"BCT3293","SOT23-6","8路串联共阳",null,"KTD256替代方案"]
[]
[null,"第三类  BCT2XXX  音频功放系列"]
[null,"Class AB 音频功放   Audio PA"]
[null,"BCT2890ELL-TR ","AQFN1.6x1.6-9","Class AB mono Audio PA","3K/Reel","广芯专利AQFN-9封装，完全兼容LM4990系列的CSP封装"]
[null,"BCT2010ELL-TR","AQFN1.6x1.6-9","Class D mono Audio PA","3K/Reel","广芯专利AQFN-9封装，完全兼容TPA2010系列的CSP封装"]
[null,"BCT2145ELL-TR","AQFN1.6x1.6-9","Class D mono Audio PA with AGC ","3K/Reel","广芯专利AQFN-9封装，内置AGC功能，防止破音"]
[]
[null,"第四类  BCT5xxx  LED Panel Driver"]
[null,"BCT5024EAB","SOP24 ","16位元等电流LED驱动器","3K/Reel"]
[null,"BCT5026EAB","SOP24 ","16位元等电流LED驱动器","3K/Reel"]
[]
[null,"第五类 小家电温控系列"]
[null,"BCT530x","SOP-8","MCH陶瓷发热体温度控制芯片","3K/Reel"]
[null,"BCT535x","SOP-24","带LCD显示功能的MCH陶瓷发热体温度控制芯片","3K/Reel"]
[]
[null,"第六类 高压控制系列"]
[null,"BCT3536","SOP-8","40V DC-DC降压转换器","3K/Reel"]
[null,"BCT3538","SOP-8","单通道半桥MOSFET驱动","3K/Reel"]
[null,"BCT3540","SOP-24","三通道半桥MOSFET驱动","3K/Reel"]
[null,"广芯代理商，主营产品："]
[]
[null,"MIPI开关：BCT634，BCT636，BCT642A，BCT644，BCT644B，BCT644C，BCT646，BCT646B，BCT646C，BCT660"]
[]
[null,"模拟开关：BCT4157，BCT4257，BCT4223，BCT4221，BCT4221A，BCT4222A，BCT4222B，BCT4222C，BCT4227，BCT4228，BCT4699，BCT4899，BCT4330，BCT44600，BCT44602，BCT44603，BCT4340，BCT4350，BCT4567，BCT4567A，BCT48752，BCT48751"]
[]
[null,"USB Tyoe-C/Audio开关：BCT4480，BCT4321N，BCT4153"]
[]
[null,"Audio PA：BCT8002，BCT8002H，BCT8890，BCT8890H，BCT8005，BCT8933，BCT8937S，BCT89317，BCT89318"]
[]
[null,"CMOS OPA:BCT8721，BCT8721B，BCT8722，BCT8724，BCT8321，BCT8321B，BCT8358，BCT8324"]
[]
[null,"FM LNA：BCT5007"]
[]
[null,"充电器:BCT24157，BCT24157D，BCT24296，BCT24056，BCT4056，BCT4054，BCT4057，BCT40561，BCT40541，BCT40571"]
[]
[null,"LDO低电压：BCT2036，BCT2901，BCT2020，BCT2038，BCT2193，BCT2211，BCT2561，BCT2562，BCT2040，BCT2057，BCT2160，BCT2910，BCT2186"]
[]
[null,"LDO高电压：BCT2014，BCT2203，BCT78L0***，BCT78L05E"]
[]
[null,"OVP：BCT72901，BCT72902，BCT72905，BCT72801，BCT72802，BCT72805"]
[]
[null,"Load开关：BCT6553"]
[]
[null,"DC-DC转换器：BCT1013，BCT12568，BCT12569，BCT1810，BCT1812，BCT1813，BCT1814，BCT1815，BCT1820，BCT1821，BCT1470，BCT1471"]
[]
[null,"FLASH LED驱动：BCT3140"]
[]
[null,"白光LED驱动(连续):BCT3692B，BCT3756，BCT3401"]
[]
[null,"白光LED驱动(平行):BCT3220，BCT3256"]
[]
[null,"Funlight LED驱动：BCT3119，BCT3288A，BCT3656，BCT3299，BCT3024，BCT3236"]
[]
[null,"Dispiay LED驱动：BCT3616，BCT3617，BCT3618，BCT3620，BCT3620B，BCT3622，BCT3668，BCT3668A，BCT3628，BCT3628A，BCT3627，BCT3623，BCT3624，BCT3629A，BCT3629B，BCT3629C，BCT3629D，BCT3638，BCT3639，BCT3640，BCT3932"]
[]
[null,"双向电平转换器：BCT0102，BCT0104"]
[]
[null,"双SIM卡控制器：BCT4302B"]
[]
[null,"AC-DC转换器：BCT5034，BCT5055"]
[]
[null,"无源红外控制器：BCT0001"]
[]
[null,"烤面包机控制器：BCT5512"]