{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["第1页","第2页"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第1页","index":0,"n_rows":40,"n_cols":36,"rows_kept":40,"merged":[[0,0,40,0],[0,1,0,31],[0,32,40,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,19,1],[9,3,9,8],[9,9,9,12],[9,16,9,25],[9,26,9,31],[10,3,10,8],[10,9,10,12],[10,16,10,25],[10,26,10,31],[11,3,11,8],[11,9,11,12],[11,16,11,25],[11,26,11,31],[12,3,12,8],[12,9,12,12],[12,26,12,31],[13,3,13,8],[13,9,13,12],[13,26,13,31],[14,3,14,8],[14,9,14,12],[14,26,14,31],[15,3,15,8],[15,9,15,12],[15,16,15,25],[15,26,15,31],[16,3,16,8],[16,9,16,12],[16,16,16,25],[16,26,16,31],[17,3,17,8],[17,9,17,12],[17,16,17,25],[17,26,17,31],[18,3,18,8],[18,9,18,12],[18,16,18,25],[18,26,18,31],[19,3,19,8],[19,9,19,12],[19,16,19,25],[19,26,19,31],[20,1,39,1],[20,3,20,8],[20,9,20,12],[20,16,20,25],[20,26,20,31],[21,3,21,8],[21,9,21,12],[21,16,21,25],[21,26,21,31],[22,3,23,4],[22,5,22,8],[22,9,22,12],[22,26,22,31],[23,5,23,8],[23,9,23,12],[23,26,23,31],[24,3,25,4],[24,5,24,8],[24,9,24,12],[24,26,24,31],[25,5,25,8],[25,9,25,12],[25,26,25,31],[26,3,26,8],[26,9,26,12],[26,26,26,31],[27,2,30,2],[27,3,30,4],[27,5,29,5],[27,6,27,8],[27,9,27,12],[27,26,27,31],[28,6,28,8],[28,9,28,12],[28,26,28,31],[29,6,29,8],[29,9,29,12],[29,26,29,31],[30,5,30,8],[30,9,30,12],[30,26,30,31],[31,2,32,2],[31,3,32,4],[31,5,31,8],[31,9,31,12],[31,26,31,31],[32,5,32,8],[32,9,32,12],[32,26,32,31],[33,2,34,2],[33,3,34,4],[33,5,33,8],[33,9,33,12],[33,26,33,31],[34,5,34,8],[34,9,34,12],[34,26,34,31],[35,2,36,2],[35,3,36,4],[35,5,35,8],[35,9,35,12],[35,26,35,31],[36,5,36,8],[36,9,36,12],[36,26,36,31],[37,2,39,2],[37,3,39,4],[37,6,37,8],[37,9,37,12],[37,26,37,31],[38,6,38,8],[38,9,38,12],[38,26,38,31],[39,5,39,8],[39,9,39,12],[39,26,39,31],[40,1,40,31]],"flags":["formulas_cached_only"]}
[]
[null,"装配式结构预制构件（进场）检验批质量验收记录"]
[null,"GD-C3-51382",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"主体结构-装配式混凝土结构",{"$nulls":4},"分项工程\r\n名称",null,null,"装配式结构"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-51382 装配式结构预制构件（进场）检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"《装配式混凝土建筑工程施工质量验收规范》DBJ/T15-171-2019"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"主控项目",1,"预制构件质量证明文件",{"$nulls":5},"第4.2.1条",{"$nulls":4},"/"]
[null,null,2,"受弯预制构件结构构件性能",{"$nulls":5},"第4.2.2条",{"$nulls":4},"/"]
[null,null,3,"预制构件混凝土强度",{"$nulls":5},"第4.2.3条",{"$nulls":4},"/"]
[null,null,4,"连接钢筋中心线位置",{"$nulls":5},2,{"$nulls":4},"/"]
[null,null,5,"连接钢筋外露长度",{"$nulls":5},"+10，0",{"$nulls":4},"/"]
[null,null,6,"灌浆套筒中心线位置",{"$nulls":5},2,{"$nulls":4},"/"]
[null,null,7,"预制构件外观质量严重缺陷",{"$nulls":5},"第4.2.5条",{"$nulls":4},"/"]
[null,null,8,"预制构件的预埋件、预留孔洞、预留钢筋的规格、数量",{"$nulls":5},"第4.2.6条",{"$nulls":4},"/"]
[null,null,9,"受力预埋件抗拔、抗剪性能",{"$nulls":5},"第4.2.7条",{"$nulls":4},"/"]
[null,null,10,"粗糙面设置",{"$nulls":5},"第4.2.8条",{"$nulls":4},"/"]
[null,null,11,"键槽数量",{"$nulls":5},"第4.2.9条",{"$nulls":4},"/"]
[null,"一般项目",1,"标识",{"$nulls":5},"第4.3.1条",{"$nulls":4},"/"]
[null,null,2,"外观质量一般缺陷",{"$nulls":5},"第9.2.6条",{"$nulls":4},"/"]
[null,null,3,"受力钢筋保护层厚度",null,"柱、梁",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,4,null,null,"板、墙",{"$nulls":3},"±3",{"$nulls":4},"/"]
[null,null,5,"纵向受力钢筋",null,"间距",{"$nulls":3},"±10",{"$nulls":4},"/"]
[null,null,6,null,null,"排距",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,7,"横向受力钢筋",{"$nulls":5},"±20",{"$nulls":4},"/"]
[null,null,8,"长度(mm)",null,"楼板、梁、柱","＜12m",null,null,"±5",{"$nulls":4},"/"]
[{"$nulls":6},"≥12m且小于18m",null,null,"±10",{"$nulls":4},"/"]
[{"$nulls":6},"≥18m",null,null,"±20",{"$nulls":4},"/"]
[{"$nulls":5},"阳台板、空调板、楼梯",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,9,"宽度(mm)",null,"楼板、梁、柱、阳台板、空调板、 楼梯",{"$nulls":3},"±5",{"$nulls":4},"/"]
[{"$nulls":5},"剪力墙",{"$nulls":3},"±4",{"$nulls":4},"/"]
[null,null,10,"高度(mm)",null,"梁、柱",{"$nulls":3},"±5",{"$nulls":4},"/"]
[{"$nulls":5},"墙板",{"$nulls":3},"±4",{"$nulls":4},"/"]
[null,null,11,"厚度(mm)",null,"楼板",{"$nulls":3},"±5",{"$nulls":4},"/"]
[{"$nulls":5},"墙板、阳台板、空调板、楼梯",{"$nulls":3},"±3",{"$nulls":4},"/"]
[null,null,12,"表面平整度(mm)",null,"内表面","楼板、墙板",null,null,4,{"$nulls":4},"/"]
[{"$nulls":5},"外表面","楼板、墙板",null,null,3,{"$nulls":4},"/"]
[{"$nulls":5},"梁、柱、阳台板、空调板、楼梯",{"$nulls":3},4,{"$nulls":4},"/"]

{"sheet":"第2页","index":1,"n_rows":45,"n_cols":36,"rows_kept":45,"merged":[[0,0,45,0],[0,1,0,31],[0,32,45,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,38,1],[9,2,10,2],[9,3,10,4],[9,5,9,8],[9,9,9,12],[9,26,9,31],[10,5,10,8],[10,9,10,12],[10,26,10,31],[11,2,12,2],[11,3,12,4],[11,5,11,8],[11,9,11,12],[11,26,11,31],[12,5,12,8],[12,9,12,12],[12,26,12,31],[13,2,14,2],[13,3,14,4],[13,5,13,8],[13,9,13,12],[13,26,13,31],[14,5,14,8],[14,9,14,12],[14,26,14,31],[15,2,16,2],[15,3,16,4],[15,5,15,6],[15,7,18,8],[15,9,15,12],[15,26,15,31],[16,5,16,6],[16,9,16,12],[16,26,16,31],[17,2,18,2],[17,3,18,4],[17,5,17,6],[17,9,17,12],[17,26,17,31],[18,5,18,6],[18,9,18,12],[18,26,18,31],[19,2,20,2],[19,3,20,4],[19,5,19,6],[19,7,20,8],[19,9,19,12],[19,26,19,31],[20,5,20,6],[20,9,20,12],[20,26,20,31],[21,2,22,2],[21,3,22,4],[21,5,21,6],[21,7,26,8],[21,9,21,12],[21,26,21,31],[22,5,22,6],[22,9,22,12],[22,26,22,31],[23,2,24,2],[23,3,24,4],[23,5,23,6],[23,9,23,12],[23,26,23,31],[24,5,24,6],[24,9,24,12],[24,26,24,31],[25,2,26,2],[25,3,26,4],[25,5,25,6],[25,9,25,12],[25,26,25,31],[26,5,26,6],[26,9,26,12],[26,26,26,31],[27,2,28,2],[27,3,28,4],[27,5,27,8],[27,9,27,12],[27,26,27,31],[28,5,28,8],[28,9,28,12],[28,26,28,31],[29,2,30,2],[29,3,30,4],[29,5,29,8],[29,9,29,12],[29,26,29,31],[30,5,30,8],[30,9,30,12],[30,26,30,31],[31,2,32,2],[31,3,32,4],[31,5,31,8],[31,9,31,12],[31,26,31,31],[32,5,32,8],[32,9,32,12],[32,26,32,31],[33,3,33,4],[33,5,33,8],[33,9,33,12],[33,26,33,31],[34,2,35,2],[34,3,35,4],[34,5,34,8],[34,9,34,12],[34,26,34,31],[35,5,35,8],[35,9,35,12],[35,26,35,31],[36,2,38,2],[36,3,38,4],[36,5,36,8],[36,9,36,12],[36,26,36,31],[37,5,37,8],[37,9,37,12],[37,26,37,31],[38,5,38,8],[38,9,38,12],[38,26,38,31],[39,1,41,5],[39,6,41,15],[39,16,41,16],[39,17,39,21],[39,22,39,31],[40,17,40,21],[40,22,40,31],[41,17,41,31],[42,1,44,5],[42,6,44,15],[42,16,44,16],[42,17,42,31],[43,17,43,21],[43,22,43,31],[44,17,44,31],[45,1,45,31]],"flags":["formulas_cached_only"]}
[]
[null,"装配式结构预制构件（进场）检验批质量验收记录（续表）"]
[null,"GD-C3-51382/1",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"主体结构-装配式混凝土结构",{"$nulls":4},"分项工程\r\n名称",null,null,"装配式结构"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-51382 装配式结构预制构件（进场）检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"《装配式混凝土建筑工程施工质量验收规范》DBJ/T15-171-2019"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"一般项目",13,"侧向\r\n弯曲\r\n(mm)\r\n",null,"楼板、梁、柱、阳台板、空调板、楼梯",{"$nulls":3},"L/750\r\n且≤20",{"$nulls":4},"/"]
[{"$nulls":5},"墙板",{"$nulls":3},"L/1000\r\n且≤20",{"$nulls":4},"/"]
[null,null,14,"扭翘(mm)",null,"楼板",{"$nulls":3},"L/750",{"$nulls":4},"/"]
[{"$nulls":5},"墙板",{"$nulls":3},"L/1000",{"$nulls":4},"/"]
[null,null,15,"对角线差",null,"楼板",{"$nulls":3},"6",{"$nulls":4},"/"]
[{"$nulls":5},"墙板",{"$nulls":3},"5",{"$nulls":4},"/"]
[null,null,16,"预埋钢板",null,"中心线位置",null,"楼板、墙板、 梁、柱",null,"5",{"$nulls":4},"/"]
[{"$nulls":5},"平面高差",{"$nulls":3},"0，-5",{"$nulls":4},"/"]
[null,null,17,"预埋螺栓",null,"中心线位置",{"$nulls":3},"2",{"$nulls":4},"/"]
[{"$nulls":5},"外露长度",{"$nulls":3},"+10，-5",{"$nulls":4},"/"]
[null,null,18,"预留套筒、螺母",null,"中心线位置",null,"墙板",null,"2",{"$nulls":4},"/"]
[{"$nulls":5},"平面高差",{"$nulls":3},"0，-5",{"$nulls":4},"/"]
[null,null,19,"预留钢筋",null,"中心线位置",null,"楼板、墙板、 梁、柱",null,"3",{"$nulls":4},"/"]
[{"$nulls":5},"外露长度",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,20,"预留孔",null,"中心线位置",{"$nulls":3},"5",{"$nulls":4},"/"]
[{"$nulls":5},"孔尺寸",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,21,"预留洞",null,"中心线位置",{"$nulls":3},"5",{"$nulls":4},"/"]
[{"$nulls":5},"洞口尺寸、深 度",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,22,"预埋吊环",null,"中心线位置",{"$nulls":3},"10",{"$nulls":4},"/"]
[{"$nulls":5},"留出高度",{"$nulls":3},"0，-10",{"$nulls":4},"/"]
[null,null,23,"预埋套管",null,"中心线位置",{"$nulls":3},"5",{"$nulls":4},"/"]
[{"$nulls":5},"与混凝土面平面高差",{"$nulls":3},"5，10",{"$nulls":4},"/"]
[null,null,24,"预埋线盒",null,"中心线位置",{"$nulls":3},"10",{"$nulls":4},"/"]
[{"$nulls":5},"与混凝土面平面高差",{"$nulls":3},"0，-5",{"$nulls":4},"/"]
[null,null,25,"预埋线管",null,"管口外露长度",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,null,26,"粗糙面凹凸深度",null,"叠合板面、叠合梁面",{"$nulls":3},"≥4",{"$nulls":4},"/"]
[{"$nulls":5},"梁端、柱端、墙端",{"$nulls":3},"≥6",{"$nulls":4},"/"]
[null,null,27,"键槽",null,"中心线位置",{"$nulls":3},"5",{"$nulls":4},"/"]
[{"$nulls":5},"长度、宽度",{"$nulls":3},"±5",{"$nulls":4},"/"]
[{"$nulls":5},"深度",{"$nulls":3},"±5",{"$nulls":4},"/"]
[null,"施工单位\r\n检查结果",{"$nulls":15},"施工员："]
[{"$nulls":17},"质量员："]
[{"$nulls":17},"年  月  日"]
[null,"监理单位\r\n验收结论"]
[{"$nulls":17},"专业监理工程师："]
[{"$nulls":17},"年  月  日"]