{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["第1页"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第1页","index":0,"n_rows":35,"n_cols":36,"rows_kept":35,"merged":[[0,0,35,0],[0,1,0,31],[0,32,35,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,11,1],[9,3,9,8],[9,9,9,12],[9,16,9,25],[9,26,9,31],[10,3,10,8],[10,9,10,12],[10,16,10,25],[10,26,10,31],[11,3,11,8],[11,9,11,12],[11,16,11,25],[11,26,11,31],[12,1,28,1],[12,3,12,8],[12,9,12,12],[12,16,12,25],[12,26,12,31],[13,3,13,8],[13,9,13,12],[13,16,13,25],[13,26,13,31],[14,2,25,2],[14,3,25,3],[14,4,19,4],[14,5,15,5],[14,6,14,8],[14,9,14,12],[14,26,14,31],[15,6,15,8],[15,9,15,12],[15,26,15,31],[16,5,17,5],[16,6,16,8],[16,9,16,12],[16,26,16,31],[17,6,17,8],[17,9,17,12],[17,26,17,31],[18,5,19,5],[18,6,18,8],[18,9,18,12],[18,26,18,31],[19,6,19,8],[19,9,19,12],[19,26,19,31],[20,4,25,4],[20,5,21,5],[20,6,20,8],[20,9,20,12],[20,26,20,31],[21,6,21,8],[21,9,21,12],[21,26,21,31],[22,5,23,5],[22,6,22,8],[22,9,22,12],[22,26,22,31],[23,6,23,8],[23,9,23,12],[23,26,23,31],[24,5,25,5],[24,6,24,8],[24,9,24,12],[24,26,24,31],[25,6,25,8],[25,9,25,12],[25,26,25,31],[26,2,28,2],[26,3,28,4],[26,5,26,8],[26,9,26,12],[26,26,26,31],[27,5,28,6],[27,7,27,8],[27,9,27,12],[27,26,27,31],[28,7,28,8],[28,9,28,12],[28,26,28,31],[29,1,31,5],[29,6,31,15],[29,16,31,16],[29,17,29,21],[29,22,29,31],[30,17,30,21],[30,22,30,31],[31,17,31,31],[32,1,34,5],[32,6,34,15],[32,16,34,16],[32,17,32,31],[33,17,33,21],[33,22,33,31],[34,17,34,31],[35,1,35,31]],"flags":["formulas_cached_only"]}
[]
[null,"室内热水系统管道及配件安装检验批质量验收记录"]
[null,"GD-C3-5166",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"建筑给水排水及供暖-室内热水系统",{"$nulls":4},"分项工程\r\n名称",null,null,"管道及配件安装"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-5166 室内热水系统管道及配件安装检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"建筑给水排水及供暖施工方案/《建筑给水排水及采暖工程质量验收规范》GB50242-2002"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"主控项目",1,"热水供应系统管道水压试验",{"$nulls":5},"设计要求",{"$nulls":4},"/"]
[null,null,2,"热水供应系统管道安装补偿器",{"$nulls":5},"设计要求",{"$nulls":4},"/"]
[null,null,3,"热水供应系统管道冲洗",{"$nulls":5},"第6.2.3条",{"$nulls":4},"/"]
[null,"一般项目",1,"管道安装坡度",{"$nulls":5},"设计规定",{"$nulls":4},"/"]
[null,null,2,"温度控制器和阀门安装",{"$nulls":5},"第6.2.5条",{"$nulls":4},"/"]
[null,null,3,"管道安装偏差(mm)","水平管道纵横方向弯曲","钢管","每米",null,null,"1",{"$nulls":4},"/"]
[{"$nulls":6},"全长25m以上",null,null,"≯25",{"$nulls":4},"/"]
[{"$nulls":5},"塑料管复合管","每米",null,null,"1.5",{"$nulls":4},"/"]
[{"$nulls":6},"全长25m以上",null,null,"≯25",{"$nulls":4},"/"]
[{"$nulls":5},"铸铁管","每米",null,null,"2",{"$nulls":4},"/"]
[{"$nulls":6},"全长25m以上",null,null,"≯25",{"$nulls":4},"/"]
[{"$nulls":4},"立管垂直度","钢管","每米",null,null,"3",{"$nulls":4},"/"]
[{"$nulls":6},"5m以上",null,null,"≯8",{"$nulls":4},"/"]
[{"$nulls":5},"塑料管复合管","每米",null,null,"2",{"$nulls":4},"/"]
[{"$nulls":6},"5m以上",null,null,"≯8",{"$nulls":4},"/"]
[{"$nulls":5},"铸铁管","每米",null,null,"3",{"$nulls":4},"/"]
[{"$nulls":6},"5m以上",null,null,"≯10",{"$nulls":4},"/"]
[null,null,4,"保温层允许偏差(mm)",null,"厚度δ",{"$nulls":3},"+0.1δ\r\n-0.05δ",{"$nulls":4},"/"]
[{"$nulls":5},"表面平整度",null,"卷材",null,"5",{"$nulls":4},"/"]
[{"$nulls":7},"涂抹",null,"10",{"$nulls":4},"/"]
[null,"施工单位\r\n检查结果",{"$nulls":15},"施工员："]
[{"$nulls":17},"质量员："]
[{"$nulls":17},"年  月  日"]
[null,"监理单位\r\n验收结论"]
[{"$nulls":17},"专业监理工程师："]
[{"$nulls":17},"年  月  日"]