{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["第1页","第2页"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第1页","index":0,"n_rows":28,"n_cols":36,"rows_kept":28,"merged":[[0,0,28,0],[0,1,0,31],[0,32,28,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,12,1],[9,3,9,8],[9,9,9,12],[9,16,9,25],[9,26,9,31],[10,3,10,8],[10,9,10,12],[10,16,10,25],[10,26,10,31],[11,3,11,8],[11,9,11,12],[11,16,11,25],[11,26,11,31],[12,3,12,8],[12,9,12,12],[12,16,12,25],[12,26,12,31],[13,1,27,1],[13,3,13,8],[13,9,13,12],[13,16,13,25],[13,26,13,31],[14,2,23,2],[14,3,23,3],[14,4,15,5],[14,6,14,8],[14,9,14,12],[14,16,14,25],[14,26,14,31],[15,6,15,8],[15,9,15,12],[15,16,15,25],[15,26,15,31],[16,4,17,5],[16,6,16,8],[16,9,16,12],[16,16,16,25],[16,26,16,31],[17,6,17,8],[17,9,17,12],[17,16,17,25],[17,26,17,31],[18,4,19,5],[18,6,18,8],[18,9,18,12],[18,16,18,25],[18,26,18,31],[19,6,19,8],[19,9,19,12],[19,16,19,25],[19,26,19,31],[20,4,21,5],[20,6,20,8],[20,9,20,12],[20,16,20,25],[20,26,20,31],[21,6,21,8],[21,9,21,12],[21,16,21,25],[21,26,21,31],[22,4,23,5],[22,6,22,8],[22,9,22,12],[22,16,22,25],[22,26,22,31],[23,6,23,8],[23,9,23,12],[23,16,23,25],[23,26,23,31],[24,2,27,2],[24,3,27,3],[24,4,25,5],[24,6,24,8],[24,9,24,12],[24,16,24,25],[24,26,24,31],[25,6,25,8],[25,9,25,12],[25,16,25,25],[25,26,25,31],[26,4,27,5],[26,6,26,8],[26,9,26,12],[26,16,26,25],[26,26,26,31],[27,6,27,8],[27,9,27,12],[27,16,27,25],[27,26,27,31],[28,1,28,31]],"flags":["formulas_cached_only"]}
[]
[null,"水性涂料涂饰检验批质量验收记录"]
[null,"GD-C3-51467",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"建筑装饰装修-涂饰",{"$nulls":4},"分项工程\r\n名称",null,null,"水性涂料涂饰"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-51467 水性涂料涂饰检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"《建筑涂饰工程施工及验收规程》JGJ/T29-2015\r\n《建筑装饰装修工程质量验收标准》GB50210-2018"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"主控项目",1,"涂料品种、型号、性能",{"$nulls":5},"第12.2.1条",{"$nulls":4},"/"]
[null,null,2,"涂饰颜色、光泽、图案",{"$nulls":5},"第12.2.2条",{"$nulls":4},"/"]
[null,null,3,"涂饰质量",{"$nulls":5},"第12.2.3条",{"$nulls":4},"/"]
[null,null,4,"基层处理",{"$nulls":5},"第12.2.4条",{"$nulls":4},"/"]
[null,"一般项目",1,"与其他材料和设备衔接处",{"$nulls":5},"第12.2.8条",{"$nulls":4},"/"]
[null,null,2,"薄\r\n涂\r\n料\r\n涂\r\n饰\r\n质\r\n量\r\n允\r\n许\r\n偏\r\n差","颜色",null,"普通涂饰",null,null,"均匀一致",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"均匀一致",{"$nulls":4},"/"]
[{"$nulls":4},"光泽、光滑",null,"普通涂饰",null,null,"光泽基本均匀，光滑无挡手感",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"光泽均匀一致，光滑",{"$nulls":4},"/"]
[{"$nulls":4},"泛碱、咬色",null,"普通涂饰",null,null,"允许少量\r\n轻微",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"不允许",{"$nulls":4},"/"]
[{"$nulls":4},"流坠、疙瘩",null,"普通涂饰",null,null,"允许少量\r\n轻微",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"不允许",{"$nulls":4},"/"]
[{"$nulls":4},"砂眼、刷纹",null,"普通涂饰",null,null,"允许少量轻微砂眼、刷纹通顺",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"无砂眼、\r\n无刷纹",{"$nulls":4},"/"]
[null,null,3,"厚涂料涂饰质量允许偏差","颜色",null,"普通涂饰",null,null,"均匀一致",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"均匀一致",{"$nulls":4},"/"]
[{"$nulls":4},"光泽",null,"普通涂饰",null,null,"光泽基本\r\n均匀",{"$nulls":4},"/"]
[{"$nulls":6},"高级涂饰",null,null,"光泽均匀\r\n一致",{"$nulls":4},"/"]

{"sheet":"第2页","index":1,"n_rows":27,"n_cols":36,"rows_kept":27,"merged":[[0,0,27,0],[0,1,0,31],[0,32,27,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,7],[4,8,4,12],[4,13,4,15],[4,16,4,25],[4,26,4,31],[5,1,20,1],[5,2,8,2],[5,3,8,3],[5,4,6,4],[5,5,5,7],[5,8,5,12],[5,16,5,25],[5,26,5,31],[6,5,6,7],[6,8,6,12],[6,16,6,25],[6,26,6,31],[7,4,8,4],[7,5,7,7],[7,8,7,12],[7,16,7,25],[7,26,7,31],[8,5,8,7],[8,8,8,12],[8,16,8,25],[8,26,8,31],[9,2,12,2],[9,3,12,3],[9,4,9,7],[9,8,9,12],[9,16,9,25],[9,26,9,31],[10,4,10,7],[10,8,10,12],[10,16,10,25],[10,26,10,31],[11,4,11,7],[11,8,11,12],[11,16,11,25],[11,26,11,31],[12,4,12,7],[12,8,12,12],[12,16,12,25],[12,26,12,31],[13,2,20,2],[13,3,20,3],[13,4,15,7],[13,8,13,9],[13,10,13,11],[13,12,14,12],[13,13,15,15],[13,16,15,25],[13,26,15,31],[16,4,16,7],[16,26,16,31],[17,4,17,7],[17,26,17,31],[18,4,18,7],[18,26,18,31],[19,4,19,7],[19,26,19,31],[20,4,20,7],[20,26,20,31],[21,1,23,5],[21,6,23,15],[21,16,23,16],[21,17,21,22],[21,23,21,31],[22,17,22,22],[22,23,22,31],[23,17,23,31],[24,1,26,5],[24,6,26,15],[24,16,26,16],[24,17,24,31],[25,17,25,22],[25,23,25,31],[26,17,26,31],[27,1,27,31]],"flags":["formulas_cached_only"]}
[]
[null,"水性涂料涂饰检验批质量验收记录（续）"]
[null,"GD-C3-51467/1",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"验收项目",{"$nulls":6},"设计要求及\r\n规范规定",{"$nulls":4},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"一般项目",3,"厚涂料涂饰质量允许偏差","泛碱、咬色","普通涂饰",null,null,"允许少量轻微",{"$nulls":5},"/"]
[{"$nulls":5},"高级涂饰",null,null,"不允许",{"$nulls":5},"/"]
[{"$nulls":4},"点状分布","普通涂饰",null,null,"-",{"$nulls":5},"/"]
[{"$nulls":5},"高级涂饰",null,null,"疏密均匀",{"$nulls":5},"/"]
[null,null,4,"复层涂料涂饰质量允许偏差","颜色",{"$nulls":3},"均匀一致",{"$nulls":5},"/"]
[{"$nulls":4},"光泽",{"$nulls":3},"光泽基本均匀",{"$nulls":5},"/"]
[{"$nulls":4},"泛碱、咬色",{"$nulls":3},"不允许",{"$nulls":5},"/"]
[{"$nulls":4},"喷点疏密程度",{"$nulls":3},"均匀，不允许连片",{"$nulls":5},"/"]
[null,null,5,"水性涂料涂饰允许偏差\r\n(mm)","项目",{"$nulls":3},"薄涂料",null,"厚涂料",null,"复层涂料","最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果"]
[{"$nulls":8},"普通涂饰","高级涂饰","普通涂饰","高级涂饰"]
[{"$nulls":8},"","","","",""]
[{"$nulls":4},"立面垂直度",{"$nulls":3},3,2,4,3,5,null,"/"]
[{"$nulls":4},"表面平整度",{"$nulls":3},3,2,4,3,5,null,"/"]
[{"$nulls":4},"阴阳角方正",{"$nulls":3},3,2,4,3,4,null,"/"]
[{"$nulls":4},"装饰线、分色线直线度",{"$nulls":3},2,1,2,1,3,null,"/"]
[{"$nulls":4},"墙裙、勒脚上口直线度",{"$nulls":3},2,1,2,1,3,null,"/"]
[null,"施工单位\r\n检查结果",{"$nulls":15},"施工员："]
[{"$nulls":17},"质量员："]
[{"$nulls":17},"年  月  日"]
[null,"监理单位\r\n验收结论"]
[{"$nulls":17},"专业监理工程师\r\n(建设单位项目负责人)："]
[{"$nulls":17},"年  月  日"]