{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["第1页"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"第1页","index":0,"n_rows":28,"n_cols":36,"rows_kept":28,"merged":[[0,0,28,0],[0,1,0,31],[0,32,28,32],[1,1,1,31],[2,1,2,25],[3,1,3,31],[4,1,4,3],[4,4,4,10],[4,11,4,14],[4,15,4,19],[4,20,4,22],[4,23,4,31],[5,1,5,3],[5,4,5,10],[5,11,5,14],[5,15,5,19],[5,20,5,22],[5,23,5,31],[6,1,6,3],[6,4,6,10],[6,11,6,14],[6,15,6,19],[6,20,6,22],[6,23,6,31],[7,1,7,3],[7,4,7,31],[8,1,8,8],[8,9,8,12],[8,13,8,15],[8,16,8,25],[8,26,8,31],[9,1,14,1],[9,3,9,8],[9,9,9,12],[9,16,9,25],[9,26,9,31],[10,3,10,8],[10,9,10,12],[10,16,10,25],[10,26,10,31],[11,3,11,8],[11,9,11,12],[11,16,11,25],[11,26,11,31],[12,3,12,8],[12,9,12,12],[12,16,12,25],[12,26,12,31],[13,3,13,8],[13,9,13,12],[13,16,13,25],[13,26,13,31],[14,3,14,8],[14,9,14,12],[14,16,14,25],[14,26,14,31],[15,1,21,1],[15,3,15,8],[15,9,15,12],[15,16,15,25],[15,26,15,31],[16,3,16,8],[16,9,16,12],[16,16,16,25],[16,26,16,31],[17,3,17,8],[17,9,17,12],[17,16,17,25],[17,26,17,31],[18,3,18,8],[18,9,18,12],[18,16,18,25],[18,26,18,31],[19,3,19,8],[19,9,19,12],[19,16,19,25],[19,26,19,31],[20,3,20,8],[20,9,20,12],[20,16,20,25],[20,26,20,31],[21,3,21,8],[21,9,21,12],[21,16,21,25],[21,26,21,31],[22,1,24,5],[22,6,24,15],[22,16,24,16],[22,17,22,21],[22,22,22,31],[23,17,23,21],[23,22,23,31],[24,17,24,31],[25,1,27,5],[25,6,27,15],[25,16,27,16],[25,17,25,31],[26,17,26,21],[26,22,26,31],[27,17,27,31],[28,1,28,31]],"flags":["formulas_cached_only"]}
[]
[null,"管网安装检验批质量验收记录"]
[null,"GD-C3-51635",{"$nulls":24},"0",null,"0",null,"1"]
[]
[null,"单位(子单位)\r\n工程名称",null,null,"铭智资料培训中心",{"$nulls":6},"分部(子分部)\r\n工程名称\r\n",{"$nulls":3},"建筑给水排水及供暖-自动喷水灭火系统",{"$nulls":4},"分项工程\r\n名称",null,null,"管网及系统组件安装"]
[null,"总承包\r\n施工单位",{"$nulls":9},"项目负责人",{"$nulls":8},"检验批容量"]
[null,"专业承(分)\r\n包单位",null,null,"/",{"$nulls":6},"项目负责人",{"$nulls":8},"检验批部位",null,null,"GD-C3-51635 管网安装检验批质量验收记录"]
[null,"施工、验收\r\n依据",null,null,"《自动喷水灭火系统工程施工及验收规范》GB50261-2017"]
[null,"验收项目",{"$nulls":7},"设计要求及\r\n规范规定",{"$nulls":3},"最小/实际\r\n抽样数量",null,null,"检查记录",{"$nulls":9},"检查\r\n结果",{"$nulls":6},"应测点数","合格点数","合格率"]
[null,"主控项目",1,"管网材料的选用符合相关技术标准的规定",{"$nulls":5},"第5.1.1条",{"$nulls":4},"/"]
[null,null,2,"管道连接后不应减小过水横断面面积",{"$nulls":5},"第5.1.6条",{"$nulls":4},"/"]
[null,null,3,"管网安装前及其过程中的管道校直、清除杂物及防腐处理要求",{"$nulls":5},"第5.1.10条",{"$nulls":4},"/"]
[null,null,4,"沟槽式管件及其密封件的选用、加工、连接、紧固要求",{"$nulls":5},"第5.1.11条",{"$nulls":4},"/"]
[null,null,5,"管道螺纹连接的管件选用、螺纹加工及连接紧固要求",{"$nulls":5},"第5.1.12条",{"$nulls":4},"/"]
[null,null,6,"管道连接法兰的选用及连接要求",{"$nulls":5},"第5.1.13条",{"$nulls":4},"/"]
[null,"一般项目",1,"管道安装位置符合设计或本规范要求",{"$nulls":5},"第5.1.14条",{"$nulls":4},"/"]
[null,null,2,"管道支吊架(含防晃支吊架)安装的要求",{"$nulls":5},"第5.1.15条",{"$nulls":4},"/"]
[null,null,3,"管道穿越变形缝的措施；套管安装尺寸与间隙填塞要求",{"$nulls":5},"第5.1.16条",{"$nulls":4},"/"]
[null,null,4,"横管安装的排水坡度及排水措施(装置)要求",{"$nulls":5},"第5.1.17条",{"$nulls":4},"/"]
[null,null,5,"管道的颜色标志要求",{"$nulls":5},"第5.1.18条",{"$nulls":4},"/"]
[null,null,6,"涂覆钢管、不锈钢管、铜管、氯化聚氯乙烯（PVC-C）管道的安装要求",{"$nulls":5},"第5.1.20～第5.1.23条",{"$nulls":4},"/"]
[null,null,7,"消防洒水软管的安装要求",{"$nulls":5},"第5.1.24条",{"$nulls":4},"/"]
[null,"施工单位\r\n检查结果",{"$nulls":15},"施工员："]
[{"$nulls":17},"质量员："]
[{"$nulls":17},"年  月  日"]
[null,"监理单位\r\n验收结论"]
[{"$nulls":17},"专业监理工程师："]
[{"$nulls":17},"年  月  日"]